**Price Schedule for Goods Offered from Within the Philippines**

***[shall be submitted with the Bid if bidder is offering goods from within the Philippines]***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**For Goods Offered from Within the Philippines**

Name of Bidder \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Project ID No.\_\_\_\_\_\_\_\_\_ Page \_\_\_of\_\_\_

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **10** |
| **Item** | **Description** | **Country of origin** | **Quantity** | **Unit price exw per item** | **Transportation and all other costs incidental to delivery, per item** | **Sales and other taxes payable if Contract is awarded, per item** | **Cost of Incidental Services, if applicable, per item** | **Total Price, per unit****(col 5+6+7+8)** | **Total Price delivered Final Destination****(col 9) x** **(col 4)** |
|  | **LOT 1: Internal Data/Buffer System** |  |  |  |  |  |  |  |  |
| 1 | **Specifications:*** **1 x Network Attached Storage (NAS)**
	+ Intel Xeon D-1521 4-core 2.4 (base) / 2.7 (turbo) GHz
	+ 32GB DDR4 ECC UDIMM
	+ 12 Drive Bays
	+ At least 4 x RJ-45 1GbE LAN Port (with link aggregation / failover support)
	+ At least 2 x USB 3.2 Gen 1 Port
	+ At least 2 x Expansion Port
	+ 2U form factor
	+ Must be compatible with DSM (DiskStationManager) Software
	+ Must be rack-mountable
	+ 500W Power Supply Unit / Adapter
	+ Environment: RoHS Compliant
	+ Certification: FCC, CE, BSMI, EAC, CCC, VCCI, RCM
* **1 x Sliding Rail Kit**
	+ Sliding rack rails must be compatible with NAS
* **12 x 3.5" HDD for NAS**
	+ At least 16TB, 7,200 rpm, 6.0Gpbs
	+ Buffer size of 512 MiB
	+ must be compatible with NAS
* **1 x M.2 SSD & 10GbE Combo Adapter Card**
	+ 10GBASE-T and M.2 SSD cache adapter
	+ must be compatible with NAS
	+ 2 x slots for 22110/2280 M.2 SSD form factor
	+ 10Gbps data transfer rate
	+ must be compliant with IEEE 802.3x/u/ab/bz/an
* **1 x M.2 NVMe SSD (for caching)**
	+ 400Gb NVMe SNV3510 Series (must be M.2 NVMe SSD Adapter compatible)
	+ must be compatible with the combo adapter card
	+ must be compatible with NAS

**Inclusions:*** At least 5 years warranty
* Inclusive of installation, configuration, knowledge transfer, service and delivery fees, and all other charges

**Additional Requirement:**1. Brochure of equipment/item, specifying its make/model/unit number and specifications. If possible, include performance metrics/reviews, establishing reliability and credibility of the product.
 |  |  |  |  |  |  |  |  |

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Legal Capacity: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Duly authorized to sign the Bid for and behalf of: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_